CENTOS 系统 ADSL 拨号连接教程
1, 先连接进入到服务器


2. 设置ADSL 拨号

adsl-setup   输入回车

[image: image1.png]login as: root
0016222, 174. 201. 210° 5 password:

Last Togin: Sun Mlay 1 22:30:55 2016

[root@cloud “J# adsl-setup <

[Welcone to the PFPOE client setwp. First, I will run some checks on
your system to make sure the PFPol client is installed properly...

JLOGIN NAME
Enter your Login Name (default root): B 33 HLE A/RADSLIK S




seth0   输入回车

[image: image2.png][LNTERFACE

Enter the Ethernet interface connected to the PPPOE modem
For Solaris, this is likely to be something like /dev/hme0.
For Linux, it will be eth, where ‘X is a mmber.

(default etho

XEAsethORFEE




[image: image3.png]Do you want the link to come up on demand, or stay wp continuously?
[f you want it to come up on demand, enter the idle time in seconds
after which the link should be dropped. If you want the link to
stay up permanently, enter “no’ (two letters, lower—case.)

NOTE: Demand-activated links do not interact well with dynamic IP
addresses. You may have some problems with demand-activated links.

[Erter the demand value (default no): []
HiEEE




DNS 直接回车就行, 如何知道也可以写上 
[image: image4.png]wis

Flease enter the IP address of your ISP s primary DNS server.

1£ your ISP clains that * the server will provide dymamic DNS addresses’,
enter server’ (all lower-case) here.

1 you just press enter, I will assume you know what you are

doing and not medify your DNS setup.

[Enter the DNS information here: [J HEAE




密码直接输入两次

[image: image5.png]PASSHORD

Please enter your Password: HAFRADSL &8, RIS EI%E

Flease re-enter your Password:




这里是否允许其它用户连接,输入 no

[image: image6.png]USERCTRL

Flease enter “yes’ (three letters, lower—case.) if you want to alluV
hormal user to start or stop DSL connection (default ves): no[|





防火墙为里输入0

[image: image7.png]FIREWALLING

Please choose the firewall rules to use. Note that these rules are
very basic. You are strongly encouraged to use a more sophisticated
firewall setup; however, these will provide basic security. If you
are running any servers on your machine, you must choose NONE' and
set up firewalling yourself. Otherwise, the firewall rules will deny
access to all standard servers like Web, e-mail, fip, etc. If you
are using SSH, the rules will block outgoing SSH comections which
allocate a privileged source port.

The firewall choices are:

0 - NONE: This script will not set any firewall rules. You are responsible
for ensuring the security of your machine. You are STRONGLY
recommended to use some kind of firewall rules.

Appropriate for a basic stand-alone web-surfing workstation

: Appropriate for a machine acting as an Internet gateway

for & LAN
Choose a tvoe of Birowal (0-2): oB&”  HAOREEZE





开机自动连接 yes

[image: image8.png]Start this comnection at boot time -
FHLEZNE{TE R, il ves

Do you want to start this comnection at boot time?

IPlease enter no or yes (default no):ves[]€—





确认刚才所有的信息,没问题直接输入y回车

[image: image9.png]e+ Summary of what you entered #

Fthernet Interface: seth)

User name: 63Lal 4— ADSL f
ictivate-on-demand: No LA
Diis : Do not adjust

Firenalline: NONE .
User Contral: 1o EEREH, fiAyEE

liccept these settings and adjust configuration files (v/n)? vl €




[image: image10.png]Congratulations, it should be all set up! HILX A TR R E R

Type * /sbin/ifup ppp0’ to bring up your ¥DSL link and */sbin/ifdown ppp0
to bring it dom.

Type * /sbin/pppoe-status /etc/sysconfiz/network-scripts/ifcfg-ppp0’

to see the link status.




3 启动ADSL连接

adsl-start   回车

[image: image11.png][rootBeloud jz Ijadsl start i A S5 LR, BB SIRRRFRRERI

[root@cloud "]




4. 简单验证下是不是能上外网
ping -c 3 www.baidu.com
[image: image12.png][rootBcloud "J# ping —c 3 www. baidu, com

PING winr. a. shifen. com (180, 97.33.108) 56(34) bytes of data.
64 bytes from 180, 97.33.108: icmp_seq=l tt
64 bytes from 180.97.33. 108 icmp_seq=2 tt
64 bytes from 180.97.33.108: icnp_seq=3 t11=55 tine=38.0 ms

—— . 2. shifen. con ping statistics —

3 packets transmitted, 3 received, 0% packet loss, time 2043ms
rtt min/ave/max/mdev = 36.673/37. 873/38. 942/0. 944 ms
[rootecloud “J# []




